Job Safety Analysis (JSA)
A JSA breaks one task into steps, lists the hazards at each step, rates the risk before and after controls, and records who applies each control. No WHS law requires a JSA by name, but it is a practical record of how you manage the risks of the task. If any box in section 2 applies, the task is high risk construction work and needs a SWMS (WHS Regulations provision 299; OHS Regulations 2017 reg 327 in Victoria), not only a JSA.
1. Task details
	Company (PCBU) name
	

	ABN
	

	Site / project address
	

	Task or job being analysed
	

	Date
	

	Supervisor
	

	Prepared by (name and position)
	

	Workers consulted in preparing this JSA
	

	Permits or licences needed for this task
	

	Plant, equipment and materials
	


2. Is this high risk construction work? (WHS Regulations provision 291; s 291 in NSW)
If ANY box applies, stop: this task needs a SWMS before work starts, not just a JSA.
	[  ]  Risk of a person falling more than 2 metres
	[  ]  Work on or near chemical, fuel or refrigerant lines

	[  ]  Work on a telecommunication tower
	[  ]  Work on or near energised electrical installations or services

	[  ]  Demolition of a load-bearing structure
	[  ]  Work in an area that may have a contaminated or flammable atmosphere

	[  ]  Work likely to disturb asbestos
	[  ]  Tilt-up or precast concrete work

	[  ]  Structural alterations or repairs requiring temporary support
	[  ]  Work on, in or adjacent to a road, railway or other traffic corridor in use

	[  ]  Work in or near a confined space
	[  ]  Work in an area with movement of powered mobile plant

	[  ]  Work in or near a shaft or trench deeper than 1.5 m, or a tunnel
	[  ]  Work in areas with artificial extremes of temperature

	[  ]  Use of explosives
	[  ]  Work in or near water with a risk of drowning

	[  ]  Work on or near pressurised gas distribution mains or piping
	[  ]  Diving work


3. Risk rating key
	Likelihood
	Consequence
	Risk level

	Almost certain
	Catastrophic
	Low

	Likely
	Major
	Medium

	Possible
	Moderate
	High

	Unlikely
	Minor
	Extreme

	Rare
	Insignificant
	


Rate each step before controls and again after controls. Risk = Likelihood x Consequence. List controls in the hierarchy of controls order: eliminate, substitute, isolate, engineering, administrative, then PPE last.
4. Job steps, hazards and controls
	Step
	Job step / task
	Hazards
	Possible consequence
	Risk before (L x C)
	Controls (in hierarchy order)
	Risk after
	Responsible person
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5. PPE and emergency
	PPE required for this task

	


	Emergency procedures, first aid and contacts

	



6. Crew sign-on
Everyone doing the task reads the JSA, raises any concerns and signs before starting. If the task, site or conditions change, stop, revise the JSA and sign again.
	Name
	Company
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	Approval
	Name and signature
	Date

	JSA prepared by

	

	


	Reviewed by (supervisor)
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